ENCE361 Emulator Note

Currently the emulator uses 1V (= 100%) for altitude, which is the same as the reference implementation of the ‘Program Demo’.

If you work with 0.8V (= 100%) than your altitude readout will differ from the emulator.